L’ANSE CREUSE PUBLIC SCHOOLS
 Pre-Owned School Bus Specifications Bid Form

 (1) 53 passenger, Type C/Special Needs Conventional Bus, 2020 or newer, with

less than 60,000 miles. Delivery required July 1, 2024 or sooner**.**

|  |  |  |
| --- | --- | --- |
|  | **MINIMUM REQUIREMENT** | **EQUIVALENT**  |
| YEAR | 2020 or newer |       |
| MILEAGE | Less than 60,000 |       |
| PASSENGER CAPACITY | 53 |       |
| HEADROOM | 78 |       |
| WHEELBASE | 218 |       |
| BRAKE TYPE | Air, ABS, Stability and Traction Control, Dust Shields |       |
| ENGINE TYPE | Detroit DD5, 5.1L, 4 Cyl, Diesel, 220 HP, 2600 RPM |       |
| FUEL TANK CAPACITY | 60 Gallon |       |
| TRANSMISSION TYPE | Automatic |       |
| AXLE, FRONT | 10,000 lb Capacity |       |
| AXLE, REAR | 17,500 lb Capacity |       |
| TIRES, FRONT | 255/70R 22.5 14 Ply Tires |       |
| TIRES, REAR | 255/70R 22.5 14 Ply Tires |       |
| SUSPENSION, FRONT | 10,000 lb |       |
| SUSPENSION, REAR | Airliner 21,000 lb |       |
| ADDITIONAL OPTIONS | (2) Roof Hatches, (4) Push-Out WindowsAir Entrance DoorVandalocks: Entrance Door and Rear Emergency DoorHeated Mirrors with Stainless Steel BracketsRadio with Inside PageStudent ReminderStrobe Light(1) 84,000 BTU Underseat HeaterDriver’s StorageAir Driver’s Seat with Right-Side ArmrestAdjustable Steering Column(3) 1131 BatteriesBackup AlarmWebasto 17,000 BTU Engine HeaterElectromagnetic On/Off Fan Drive12-Volt Power SupplyUnits Keyed AlikeTrack Seating throughout with Slide and Click tiedowns (2) includedRear AC with dash tie-in; 60,000 BTU minimum |       |
| DELIVERY CHARGES | $       | $       |
| FUEL CHARGES | $       | $       |
| **PRICE OF BUS** | **$**  | **$**  |

|  |  |
| --- | --- |
| TOTAL PRICE OF BID |  $       |