L’ANSE CREUSE PUBLIC SCHOOLS  
 Pre-Owned School Bus Specifications Bid Form

(1) 53 passenger, Type C/Special Needs Conventional Bus, 2020 or newer, with

less than 60,000 miles. Delivery required July 1, 2024 or sooner**.**

|  |  |  |
| --- | --- | --- |
|  | **MINIMUM REQUIREMENT** | **EQUIVALENT** |
| YEAR | 2020 or newer |  |
| MILEAGE | Less than 60,000 |  |
| PASSENGER CAPACITY | 53 |  |
| HEADROOM | 78 |  |
| WHEELBASE | 218 |  |
| BRAKE TYPE | Air, ABS, Stability and Traction Control, Dust Shields |  |
| ENGINE TYPE | Detroit DD5, 5.1L, 4 Cyl, Diesel, 220 HP, 2600 RPM |  |
| FUEL TANK CAPACITY | 60 Gallon |  |
| TRANSMISSION TYPE | Automatic |  |
| AXLE, FRONT | 10,000 lb Capacity |  |
| AXLE, REAR | 17,500 lb Capacity |  |
| TIRES, FRONT | 255/70R 22.5 14 Ply Tires |  |
| TIRES, REAR | 255/70R 22.5 14 Ply Tires |  |
| SUSPENSION, FRONT | 10,000 lb |  |
| SUSPENSION, REAR | Airliner 21,000 lb |  |
| ADDITIONAL OPTIONS | (2) Roof Hatches, (4) Push-Out Windows  Air Entrance Door  Vandalocks: Entrance Door and Rear Emergency Door  Heated Mirrors with Stainless Steel Brackets  Radio with Inside Page  Student Reminder  Strobe Light  (1) 84,000 BTU Underseat Heater  Driver’s Storage  Air Driver’s Seat with Right-Side Armrest  Adjustable Steering Column  (3) 1131 Batteries  Backup Alarm  Webasto 17,000 BTU Engine Heater  Electromagnetic On/Off Fan Drive  12-Volt Power Supply  Units Keyed Alike  Track Seating throughout with Slide and Click tiedowns (2) included  Rear AC with dash tie-in; 60,000 BTU minimum |  |
| DELIVERY CHARGES | $ | $ |
| FUEL CHARGES | $ | $ |
| **PRICE OF BUS** | **$** | **$** |

|  |  |
| --- | --- |
| TOTAL PRICE OF BID | $ |