**BID SPECIFICATIONS**

**L’Anse Creuse Public Schools is accepting sealed bids for Pre-Owned School Buses.**

**(1) 53-passenger Type C / Special Needs Conventional Buses, 2020 or newer, with less than 60,000 miles.**

**Minimum required specifications for the bus(s):**

|  |  |
| --- | --- |
| **Year:** | 2020 or Newer |
| **Passenger Capacity:** | 53 / 22 + (2) Wheelchairs – expandable to (5) Wheelchairs |
| **Headroom:** | 78 |
| **Wheelbase:** | 218” |
| **Brake Type:** | Air, ABS, Stability & Traction Control, Dust Shields |
| **Engine Type:** | Detroit DD5, 5.1L, 4 Cyl, Diesel, 220 HP, 2600 RPM |
| **Fuel Tank Capacity:** | 60-Gallon |
| **Transmission Type:** | Automatic |
| **Axle, Front:** | 10000-Lb Capacity |
| **Axle, Rear:** | 17500-Lb Capacity |
| **Tires, Front:** | 255/70R 22.5 14 Ply Tires |
| **Tires, Rear:** | 255/70R 22.5 14 Ply Tires |
| **Suspension Front:** | 10000-Lb |
| **Suspension Rear :** | Airliner 21000-Lb |
| **Additional Options :** | (2) Roof Hatches, (4) Push-Out Windows  Air Entrance Door  Vandalocks: Entrance Door and Rear Emergency Door  Heated Mirrors with Stainless Steel Brackets  Radio with Inside Page  Student Reminder  Strobe Light  (1) 84,000 BTU Underseat Heater  Driver’s Storage  Air Driver’s Seat with Right-Side Armrest  Adjustable Steering Column  (3) 1131 Batteries  Backup Alarm  Webasto 17,000 BTU Engine Heater  Electromagnetic On/Off Fan Drive  12-Volt Power Supply  Units Keyed Alike  Track Seating throughout with Slide and Click tiedowns (2) included  Rear AC with dash tie-in; 60,000 BTU minimum |