**BID SPECIFICATIONS**

**L’Anse Creuse Public Schools is accepting sealed bids for Pre-Owned School Buses.**

**(1) 53-passenger Type C / Special Needs Conventional Buses, 2020 or newer, with less than 60,000 miles.**

**Minimum required specifications for the bus(s):**

|  |  |
| --- | --- |
|  **Year:** | 2020 or Newer |
|  **Passenger Capacity:** | 53 / 22 + (2) Wheelchairs – expandable to (5) Wheelchairs |
|  **Headroom:** | 78 |
|  **Wheelbase:** | 218” |
|  **Brake Type:** | Air, ABS, Stability & Traction Control, Dust Shields |
|  **Engine Type:** | Detroit DD5, 5.1L, 4 Cyl, Diesel, 220 HP, 2600 RPM |
|  **Fuel Tank Capacity:** | 60-Gallon |
|  **Transmission Type:** | Automatic |
|  **Axle, Front:** | 10000-Lb Capacity |
|  **Axle, Rear:** | 17500-Lb Capacity |
|  **Tires, Front:** | 255/70R 22.5 14 Ply Tires |
|  **Tires, Rear:** | 255/70R 22.5 14 Ply Tires |
|  **Suspension Front:** | 10000-Lb |
|  **Suspension Rear :** | Airliner 21000-Lb |
|  **Additional Options :** | (2) Roof Hatches, (4) Push-Out WindowsAir Entrance DoorVandalocks: Entrance Door and Rear Emergency DoorHeated Mirrors with Stainless Steel BracketsRadio with Inside PageStudent ReminderStrobe Light(1) 84,000 BTU Underseat HeaterDriver’s StorageAir Driver’s Seat with Right-Side ArmrestAdjustable Steering Column(3) 1131 BatteriesBackup AlarmWebasto 17,000 BTU Engine HeaterElectromagnetic On/Off Fan Drive12-Volt Power SupplyUnits Keyed AlikeTrack Seating throughout with Slide and Click tiedowns (2) includedRear AC with dash tie-in; 60,000 BTU minimum |