L’ANSE CREUSE PUBLIC SCHOOLS  
 Pre-Owned School Bus Specifications Bid Form

|  |  |  |
| --- | --- | --- |
|  | **MINIMUM REQUIREMENT** | **EQUIVALENT** |
| YEAR | 2021 or newer |  |
| MILEAGE | Less than 30,000 |  |
| PASSENGER CAPACITY | 77 |  |
| HEADROOM | 78 |  |
| WHEELBASE | 279 |  |
| BRAKE TYPE | Air, ABS, Stability and Traction Control, Dust Shields |  |
| ENGINE TYPE | Detroit DD5, 5.1L, 4 Cyl, Diesel, 220 HP, 2600 RPM |  |
| FUEL TANK CAPACITY | 60 Gallon |  |
| TRANSMISSION TYPE | Automatic |  |
| AXLE, FRONT | 10,000 lb Capacity |  |
| AXLE, REAR | 21,000 lb Capacity |  |
| TIRES, FRONT | Front Hankook AH24 11R22.5 14 Ply Tires |  |
| TIRES, REAR | Rear Hankook AH24 11R22.5 14 Ply Tires |  |
| SUSPENSION, FRONT | 10,000 lb |  |
| SUSPENSION, REAR | Airliner 21,000 lb |  |
| ADDITIONAL OPTIONS | (2) Roof Hatches, (4) Push-Out Windows  Air Entrance Door  Vandalocks: Entrance Door and Rear Emergency Door  Heated Mirrors with Stainless Steel Brackets  Radio with Inside Page  Student Reminder  Strobe Light  (2) 84,000 BTU Underseat Heaters  Driver’s Storage  Air Driver’s Seat with Right-Side Armrest  Adjustable Steering Column  (3) 1131 Batteries  Backup Alarm  Webasto 17,000 BTU Engine Heater  Electromagnetic On/Off Fan Drive  12-Volt Power Supply  Units Keyed Alike |  |
|  |  |  |
| DELIVERY CHARGES | $ | $ |
| FUEL CHARGES | $ | $ |
| **PRICE OF BUS** | **$** | **$** |

Two (2) 77 passenger, Type C/Conventional Buses, 2021 or newer, with less than 30,000 miles. Delivery required by July 1, 2024 or sooner.  
  
**BUS #** **MAKE/MODEL/YEAR**

|  |  |
| --- | --- |
| Bus #1 | $ |
| Bus #2 | $ |
|  |  |
| TOTAL PRICE OF BID | $ |

SUMMARY OF BID